#
REFRIGERANT PRESSURE SWITCH INSPECTION

BME074061503201

1. Install the gas charging set.

2. Disconnect the refrigerant pressure switch connector.

3. Verify the high-pressure side reading of the manifold gauge and continuity between the terminals are as shown.

  • If not as specified, replace the front cooler pipe No.2.

Type | High and low | Middle
--- | --- | ---
Triple-pressure type | B-C | A-D
Dual-pressure type | A-B | -

Triple-pressure Type

Dual-pressure Type