#
TCS OFF SWITCH INSPECTION

BME041446444202

## Switch and ABS/TCS HU/CM Harness Inspection

### A Type

1. Remove the TCS OFF switch.

2. Inspect for continuity between the TCS OFF switch terminals using an ohmmeter.

  • If not within the specification, replace the TCS OFF switch.

### B Type

1. Remove the TCS OFF switch.

2. Inspect for continuity between the TCS OFF switch terminals using an ohmmeter.

  • If not within the specification, replace the TCS OFF switch.