#
OIL COOLER REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME011114700203

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

3. Remove the oil filter cover. (See OIL FILTER REPLACEMENT [MZR-CD (RF Turbo)].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of the removal.

1 | Water hose
2 | Oil cooler

6. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

7. Inspect the oil level.

  • If necessary, add oil. (See ENGINE OIL LEVEL INSPECTION.)

8. Start the engine and inspect for oil leakage.

  • If the oil leaks, specify the faulty part and repair or replace it.