#
FRONT AIR INTAKE ACTUATOR INSPECTION

BME074061060W02

1. Remove the front air intake actuator.

2. Connect battery positive voltage to terminal G and ground to terminal A or C of the front air intake actuator.

3. Verify that the front air intake actuator operates as shown below.

  • If not as specified, replace the front air intake actuator.

Connection | Movement
--- | ---
B+ | GND
G | A | FRESH→RECIRCULATE
G | C | RECIRCULATE→FRESH