#
N-D SELECT CONTROL DESCRIPTION [JA5A-EL]

BME051718901T07
• When the selector lever is switched from the P or N position to the driving ranges, or vice versa, the engine speed change is minimized by regulating fuel injection volume in order to improve select feel.
• Range signals are output to the PCM in the following instances:
When the selector lever is switched from the P or N position to the driving ranges, or vice versa, and the specified time has elapsed.
• The PCM regulates fuel injection volume based on inhibitor signals prevent change in engine speed.