#
VARIABLE VALVE TIMING ACTUATOR INSPECTION

B3E011000142201

## L3 (with variable valve timing mechanism)

  Caution

  • Variable valve timing actuator cannot be disassembled because it is a precision unit.

1. Confirm that the groove of the rotor and notch of the cover at the variable valve timing actuator are aligned and fixed.

  • If the notch and the bump are not aligned, rotate the rotor toward the valve timing retard position by hand until they are in place.
  • If the rotor and cover are not fixed even though their notch and groove are aligned, replace the variable valve timing actuator.