#
CAMSHAFT POSITION (CMP) SENSOR INSPECTION [L3]

BME014018230W01

  Caution

  • When foreign material, such as an iron chips, gets on the CMP sensor, it can cause abnormal output from the sensor because of flux turbulence and adversely affect engine control. Be sure there is no foreign material on the CMP sensor when replacing.

  Note

  • Perform the following inspection only when directed.

## Resistance Inspection

1. Disconnect the CMP sensor connector.

2. Measure the resistance between CMP sensor terminals A and B using an ohmmeter.

  • If not as specified, replace the CMP sensor.
  • If CMP sensor resistance is okay, perform the "Circuit Open/Short Inspection".

Specification

  400-550 ohms

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [L3].)

2. Inspect the following wiring harnesses for open or short. (continuity check)

### Open circuit

  • If there is no continuity, the circuit is open. Repair or replace the harness.
  - CMP sensor terminal A (harness-side) and PCM terminal 2M (harness-side)
  - CMP sensor terminal B (harness-side) and PCM terminal 2J (harness-side)

### Short circuit

  • If there is continuity, the circuit is shorted. Repair or replace the harness.
  - CMP sensor terminal A (harness-side) and power supply
  - CMP sensor terminal A (harness-side) and body GND
  - CMP sensor terminal B (harness-side) and power supply
  - CMP sensor terminal B (harness-side) and body GND