#
AUDIO UNIT CONSTRUCTION

BME092066900T01

## Structural View

.

1 | Base unit
2 | Upper module (CD player or CD changer)
3 | Lower module (cassette deck or MD player)
4 | Cover (without upper module)
5 | Cover (without upper module)
6 | Cover (with upper module)
7 | Cover (without lower module)
8 | Cover (with cassette deck)
9 | Cover (with MD player)

## Terminal Layout and Signal

Terminal | Signal
--- | ---
| 1A | Left front speaker (+)
1B | B+ (Power back up)
1C | Left front speaker (-)
1D | Right front speaker (+)
1E | Illumination (+)
1F | Right front speaker (-)
1G | Illumination (-)
1H | Ant. SW
1I | -
1J | AMP. control
1K | -
1L | H/F TEL mute
1M | -
1N | Steering switch
1O | -
1P | Steering switch
1Q | -
1R | ACC
1S | Left rear speaker (+)
1T | -
1U | Left rear speaker (-)
1V | Right rear speaker (+)
1W | Ground
1X | Right rear speaker (-)
| 2A | Ground (power)
2B | System mute
2C | Right input (+)
2D | Right input (-)
2E | Left input (+)
2F | Left input (-)
2G | Signal ground
2H | Input video
2I | Video ground
2J | TNS (+)
2K | Bus (-)
2L | Bus (+)
2M | TV bus (+)
2N | TV bus (-)
2O | ACC
2P | B+