#
SECOND-ROW SEAT INSTALLATION

BME09135720X202

## TYPE A

1. Set the seat's strikers on the rear floor anchor loops.

2. Lower the seat forward to lock the front strikers.

3. Supporting the seat with your hands, slowly lower the seat back rearwards to lock it in place.

4. Raise the recliner lever and raise the seat back upright.

5. Inspect the seat to ensure it is firmly locked in place.

## TYPE B

1. Install in the reverse order of removal.

## TYPE C

1. Set the seat's strikers on the front floor anchors.

2. Supporting the seat with your hands, slowly lower the seat back rearwards to lock it in place.

3. Raise the recliner lever and raise the seat back upright.

4. Inspect the seat to ensure it is firmly locked in place.