#
PLASTIC PARTS HEAT RESISTING TEMPERATURE

BME098050000B01

No. | Part Name | Code | Material Name | Heat resisting Temperature°C {°F}
--- | --- | --- | --- | ---
1 | FRONT WINDOW UPPER MOULDING | PVC | POLYVINYLCHLORIDE | 95 {203}
2 | COWL GRILLE | PP | POLYPROPYLENE | 110 {230}
3 | FRONT COMBINATION LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PP | POLYPROPYLENE | 130 {266}
4 | FRONT BUMPER | PP | POLYPROPYLENE | 100 {212}
5 | RADIATOR GRILLE (Sports type) | UPPER | PC-ABS | POLYCARBONATE-ABS | 80 {176}
LOWER | PC-ABS | POLYCARBONATE-ABS | 80 {176}
RADIATOR GRILLE (Standard type) | UPPER | ABS | ABS | 70 {158}
LOWER | ABS | ABS | 70 {158}
LOWER MOLDING (Coated) | ABS | ABS | 70 {158}
LOWER MOLDING (Material color) | AAS | AAS | 80 {178}
6 | FRONT SIDE TURN LIGHT | LENS | PMMA | ACRYLIS | 100 {212}
HOUSING | PC-PBT | POLYCARBONATE-PBT | 110 {230}
7 | OUTER HANDLE | PC | POLYCARBONATE | 130 {266}
8 | ROOF MOULDING | PET-PBT | POLYTHYLENETEPHTHALATE-PBT | 100 {212}
9 | OUTSIDE MIRROR | AAS | AAS | 80 {176}
10 | SIDE PROTECTOR | PVC | POLYVINYLCHLORIDE | 50 {122}
11 | RAIL PROTECTOR | PC-PET | POLYCARBONATE-PET | 120 {248}
12 | REAR BUMPER | PP | POLYPROPYLENE | 100 {212}
13 | REAR COMBINATION LIGHT | LENS | PMMA | ACRYLIS | 100 {212}
HOUSING | AES | AES | 100 {212}
14 | LIFTGATE GARNISH | ABS | ABS | 70 {158}
15 | REAR WINDOW MOLDING | PVC | POLYVINYLCHLORIDE | 95 {203}
16 | HIGH-MOUNT BRAKE LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PC | POLYCARBONATE | 130 {266}

  Note

  • The application of temperatures higher than heat resisting temperatures may result in part deformation.