#
SECONDARY SHAFT COMPONENTS PREINSPECTION

BME051517301M01

## 1st Gear End Play

1. Set up the secondary shaft component, and fix it.

2. Slide the 1st gear up and down, and measure the length of the movement.

  • If not within the specification, assemble the secondary shaft component again.

Length of the movement

  0.20-0.30 mm {0.0078-0.0118 in}

## 2nd Gear End Play

1. Set up the secondary shaft component, and fix it.

2. Slide the 2nd gear up and down, and measure the length of the movement.

  • If not within the specification, assemble the secondary shaft component again.

Length of the movement

  0.06-0.16 mm {0.0024-0.0063 in}