#
TRANSMISSION/TRANSAXLE FEATURES

BME050000000T02

CLUTCH
Improved operability | • Hydraulic clutch control mechanism used
Improved reliability | • Adoption of a clutch master cylinder with a one-way valve (G15M-R)
Reduced noise and vibration | • The flywheel with a damper has been adopted (A65M-R)
MTX [G15M-R]
Improved operability | • Bushings mounted on shift rod sliding surface • Equal-rigidity shift fork adopted
Reduced noise | • Larger final gear adopted
Improved reliability | • Optimized clutch housing oil lubrication groove shape adopted • Large-capacity oil passage and rear cover funnel adopted • Four-pinion gear type differential adopted • Double engagement prevention mechanism (interlock mechanism) adopted
Mis-shift prevention | • Cam-type reverse lock-out mechanism adopted
MTX [A65M-R]
Improved operability | • Cable type operation system adopted • A constant mesh type shift assist adopted