#
CYLINDER BLOCK INSPECTION

A6E242410300E01

1.• Measure the distortion of the cylinder block top surface in the six directions as indicated in the figure.

  • If the distortion exceeds the maximum, replace the cylinder block.

  Maximum cylinder block distortion:
  0.10 mm {0.004 in}

2. Measure the cylinder bores in X and Y directions at 42 mm {1.65 in} below the top surface.

  • If the cylinder bore exceeds the wear limit, replace the cylinder block.

  Standard diameter limit
  L8:
  83.000-83.030 mm {3.2677-3.2689 in}
  LF, L3, L3 (with variable valve timing mechanism):
  87.500-87.530 mm {3.4449-3.4460 in}
  Minimum / maximum bore diameter limit
  L8:
  82.940-83.090 mm {3.2653-3.2712 in}
  LF, L3, L3 (with variable valve timing mechanism):
  87.440-87.590 mm {3.4425-3.4484 in}