#
GENERATOR REMOVAL/INSTALLATION [L3]

BME011718300W01

  Warning

  • When the battery cables are connected, touching the vehicle body with generator terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the battery before performing the following operation.

  Caution

  • The generator can be damaged by the heat from the exhaust manifold. Make sure the generator duct and the generator heat insulator are installed securely.

1. Disconnect the negative battery cable.

2. Remove the splash shield.

3. Remove the transverse member. (See TRANSVERSE MEMBER REMOVAL/INSTALLATION.)

4. Remove the drive belt. (See DRIVE BELT REPLACEMENT [L3].)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

.

1 | Generator duct
2 | Terminal B wire
3 | Connector
4 | Generator heat insulator
5 | Generator (See Generator Installation Note.)

## Generator Installation Note

1. Tighten the bolt A temporary.

2. Tighten the bolt in the order B, A, and C.