#
REAR FLOOR COVERING REMOVAL/INSTALLATION

BME091768691W01

## Fixed type Second-Row Seat

1. Remove the third-row seat.

2. Remove the trunk side trim.

3. Remove the lower anchor installation bolt of the third-row seat belt.

4. Remove the trunk board.

5. Remove the fasteners.

6. Remove the rear floor covering.

7. Install in the reverse order of removal.

## Side-Sliding type Second-Row Seat

1. Remove the rear side trim.

2. Lift the third-row seat back and lower it into cargo well.

3. Remove the fastener A.

4. Return the third-row seat to its original position.

5. Remove the lower anchor installation bolt of the center third-row seat belt.

6. Remove the fasteners B.

7. Remove the ring of the cargo net, and remove the rear floor covering.

8. Install in the reverse order of removal.