#
SUPPLY PUMP CONSTRUCTION [MZR-CD (RF Turbo)]

BME011413350T03
• The pump is composed of: a feed pump that siphons fuel from the fuel tank into the supply pump, a suction control valve that controls the intake amount of fuel to the pump chamber, a delivery valve that pressure feeds fuel to the common rail, and a pump body.
• The pump body is composed of a camshaft, outer cam and plunger.
• The pump is driven by the engine. A pulley on the front end of the pump is connected to the crankshaft via a belt, thus engine torque is transmitted to the outer cam.
• Two plungers are attached in opposing pairs on the outside of the outer cam. One is used for the intake stroke and the other is for the pressure feed stroke.
• The regulator valve regulates the fuel pressure within the pump and returns fuel to the fuel tank.

.

1 | Fuel tank
2 | Fuel filter
3 | Feed pump
4 | Regulator valve
5 | Suction control valve
6 | Plunger
7 | Inflow orifice
8 | Outflow orifice
9 | Common rail
10 | Fuel injector
11 | Camshaft
12 | Main fuel flow
13 | Return fuel flow