#
THEFT-DETERRENT CONTROL MODULE REMOVAL/INSTALLATION

BME091467790201

  Note

  • Because the lock section of the module is damaged easily, do not remove the module from the bracket unless replacement is necessary. Always perform an inspection of the theft-deterrent control module before removal.

1. Disconnect the negative battery cable.

2. Remove the bracket.

3. Disconnect the theft-deterrent control module connector.

4. Remove the theft-deterrent control module by prying the lock section of the side part with a flathead screwdriver.

5. Install in the reverse order of removal.