#
FRONT BLOWER RELAY REMOVAL/INSTALLATION

BME074061691201

  Note

  • Because the lock section of the relay is damaged easily, do not remove the front blower relay from the bracket unless replacement is necessary. Always perform an inspection of the front blower relay before removal.

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Bracket
2 | Connector
3 | Front blower relay