#
OIL FILTER CONSTRUCTION [L3]

BME011114300T01
• The oil filter is attached to the right side of the oil level gage (oil pan side) on cylinder block.
• The oil filter adapter has been adopted for weight reduction. The oil pressure switch is installed on the oil filter adapter.
• A resin oil filter has been adopted for weight reduction. A drain plug has been installed on the bottom of the oil filter to improve replacement serviceability.
• An environment-friendly oil filter made of incinerable polyester has been adopted. Only filter paper needs to be replaced.
• A water-cooled oil cooler has been adopted to reduce the engine oil degradation. Also, the exclusive use oil filter adapter has been adapted for the oil cooler.

OIL FILTER SPEC.

Outer diameter | (mm {in}) | 64.9-65.0 {2.555-2.559}
Height | (mm {in}) | 73.4-73.6 {2.88-2.90}

.

1 | To water outlet case
2 | Oil cooler
3 | O-ring
4 | Oil filter adapter
5 | Oil pressure switch
6 | To thermostat
7 | Diameter
8 | Height
9 | Oil filter
10 | Oil filter cover
11 | Oil filter drain plug

.

1 | Sectional view
2 | Oil filter
3 | Oil filter bypass valve
4 | Oil filter cover
5 | Normal
6 | Bypass
7 | Spring
8 | Oil pressure
9 | Oil passage