#
DTC P0328 [L3]

BME010200300216

DTC P0328 | Knock sensor circuit high input
--- | ---
DETECTION CONDITION | • PCM monitors input signal from knock sensor when engine is running. If input voltage at PCM terminals between 2P and 2S is excessively high, PCM determines that knock sensor circuit has malfunction. Diagnostic support note • This is a continuous monitor (CCM).
• MIL illuminates if PCM detects the above malfunction conditions during first drive cycle.
• PENDING CODE is available if PCM detects the above malfunction condition.
• FREEZE FRAME DATA is available.
• DTC is stored in PCM memory.
POSSIBLE CAUSE | • Knock sensor malfunction • Connector or terminal malfunction • Short to power circuit in wiring between knock sensor terminal A and PCM terminal 2S • Short to power circuit in wiring between knock sensor terminal B and PCM terminal 2P

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | PERFORM DTC CONFIRMATION PROCEDURE • Perform DTC CONFIRMATION PROCEDURE. (See DTC CONFIRMATION PROCEDURE [L3].) • Is same DTC present? | Yes | Go to the next step.
No | Intermittent concern exists. Go to INTERMITTENT CONCERN TROUBLESHOOTING procedure. (See INTERMITTENT CONCERN TROUBLESHOOTING [L3].)
2 | INSPECT KNOCK SENSOR CONNECTOR TERMINAL • Turn the ignition switch off. • Disconnect knock sensor connector. • Inspect for poor connection at terminals A and B (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair terminal, then go to step 6.
No | Go to the next step.
3 | INSPECT KNOCK SENSOR • Perform knock sensor inspection. (See KNOCK SENSOR INSPECTION [L3].) • Is knock sensor normal? | Yes | Go to the next step.
No | Replace knock sensor, then go to step 6.
4 | INSPECT KNOCK SIGNAL CIRCUIT FOR SHORT TO POWER • Turn the ignition switch to the ON position (Engine off). • Measure voltage between knock sensor terminal A (wiring harness-side) and body GND and knock sensor terminal B (wiring harness-side) and body GND.
• Is there any voltage reading?
Yes
Repair or replace harness for short to power supply, then go to step 6.
No | Go to the next step.
5 | INSPECT PCM CONNECTOR • Disconnect PCM connector. • Inspect for poor connection (damaged, pulled-out terminals, corrosion, etc.). • Is there any malfunction? | Yes | Repair or replace terminal, then go to step 6.
No | Go to the next step.
6 | VERIFY TROUBLESHOOTING OF DTC P0328 COMPLETED • Make sure to connect all disconnected connectors. • Clear DTC from PCM memory using WDS or equivalent. • Perform KOEO/KOER self-test. (See KOEO/KOER SELF-TEST PROCEDURE [L3].)
• Is same DTC present?
Yes
Replace PCM, then go to the next step.
(See PCM REMOVAL/INSTALLATION [L3].)
No | Go to the next step.
7 | VERIFY AFTER REPAIR PROCEDURE • Perform "After Repair Procedure". (See AFTER REPAIR PROCEDURE [L3].) • Is there any DTC present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [L3].)
No | Troubleshooting completed.