#
SECOND-ROW SEAT BELT REMOVAL/INSTALLATION

BME081157730201

## Side

  Caution

  • The ELR has a spring that will unwind if the retractor's cover is removed. The spring cannot be rewound by hand. If this occurs, the ELR will not work properly. Therefore, do not disassemble the retractor.

1. Remove the trunk side trim.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Anchor cover
2 | Second-row seat belt

## Center

1. Remove the bolt.

2. Remove the second-row seat belt.

3. Install in the reverse order of removal.