#
COOLING FAN MOTOR REMOVAL/INSTALLATION [AJ]

BME011215025203

1. Disconnect the negative battery cable.

2. Remove the radiator grill. (See RADIATOR GRILLE REMOVAL/INSTALLATION.)

3. Remove the transverse member. (See TRANSVERSE MEMBER REMOVAL/INSTALLATION.)

4. Remove the engine mount member.

5. Remove the No.2 engine mount.

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

1 | Radiator bracket
2 | Fan control module connectors
3 | Radiator cowling
4 | Main fan
5 | Additional fan
6 | Main fan motor
7 | Additional fan motor
8 | Fan control module