#
FRONT BUMPER REMOVAL/INSTALLATION

BME091050031W01

1. Disconnect the negative battery cable.

2. Remove the radiator grille.

3. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Disconnect the front fog light connector.

5. Remove in the order indicated in the table.

1 | Bolt A
2 | Fastener
3 | Screw
4 | Bolt B
5 | Front bumper (See Front Bumper Removal Note.)

6. Install in the reverse order of removal.

## Front Bumper Removal Note

1. Pull the front bumper forward to disengage the front bumper from the bumper brackets.