#
VEHICLE SPEED SENSOR (VSS) REMOVAL/INSTALLATION [FN4A-EL]

BME051719200212

  Caution

  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to spill water or foreign material on the connector when disconnecting it.
  • If foreign material is stuck to the VSS, disturbance by magnetic flux can cause sensor output to be abnormal and thereby negatively affect control. Make sure that foreign material such as iron filings are not stuck to the VSS during installation.

1. Disconnect the negative battery cable.

2. Disconnect the VSS connector.

3. Remove the VSS.

4. Apply ATF to a new O-ring and install it on a VSS.

5. Install the VSS.

Tightening torque

  8-11 N·m {82-112 kgf·cm, 71-97 in·lbf}

6. Connect the VSS connector.

7. Connect the negative battery cable.