#
CRUISE CONTROL SWITCH INSPECTION

BME012066341201

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disconnect the audio control switch connector.

4. Measure the resistance and inspect for continuity between the cruise control switch terminals using a tester.

  • If not as specified, replace the cruise control switch.