#
SUPPLY PUMP FUNCTION [MZR-CD (RF Turbo)]

BME011413350T02
• An electrically controlled supply pump with ultra-high discharge pressure and low-drive torque has been adopted.
• The pump housing is constructed of aluminum to achieve weight reduction.
• An outer cam has been adopted, replacing the current inner cam, making ultra-high pressure of 180 MPa {1,835 kgf/cm 2, 26,107 psi} possible.
• The supply pump intakes the proper fuel amount and pressure feeds the fuel to the common rail.