#
FLASHER UNIT INSPECTION

BME091866830202

1. Remove the bracket and pull it toward you.

2. Measure the voltage at the flasher unit terminals as indicated below.

3. Disconnect the flasher unit connector before inspecting for continuity at terminal F.

  • If not as specified, inspect the parts listed under "Action."
  • If the parts and wiring harnesses are okay but the system still does not work properly, replace the flasher unit.

## Terminal Voltage Table (Reference)

Terminal | Signal | Connected to | Test condition | Voltage (V)/Continuity | Action
--- | --- | --- | --- | --- | ---
A | Power supply | HAZARD 10 A fuse | Under any condition | B+ | • Inspect HAZARD 10 A fuse • Inspect related harness
B | - | - | - | - | -
D | Turn signal light (LH) flashing | Turn signal light (LH) | Ignition switch at ON position | Turn switch (LH) on | Alternates between below 1.0 and B+ | • Inspect turn signal light (LH) • Inspect light switch • Inspect related harness
Turn switch (LH) off | Below 1.0
F | Flasher unit ground | GND | Under any condition: inspect for continuity to ground | Yes | • Inspect GND
G | Turn signal light (RH) flashing | Turn signal light (RH) | Ignition switch at ON position | Turn switch (RH) on | Alternates between below 1.0 and B+ | • Inspect turn signal light (RH) • Inspect light switch • Inspect related harness
Turn switch (RH) off | Below 1.0
H | Hazard warning switch on | Hazard warning switch | Hazard warning switch on | Below 1.0 | • Inspect hazard warning switch • Inspect related harness
Other | B+
I | Turn switch (RH) on/off | Light switch | Ignition switch at ON position and turn switch (RH) on | B+ | • Inspect light switch • Inspect related harness
Other | Below 1.0
J | Turn switch (LH) on/off | Light switch | Ignition switch at ON position and turn switch (LH) on | B+ | • Inspect light switch • Inspect related harness
Other | Below 1.0