#
CONTROL SYSTEM BLOCK DIAGRAM [L3]

BME014000000T05

1 | MAF/IAT sensor
2 | TP sensor
3 | MAP senor
4 | CMP sensor
5 | CKP sensor
6 | ECT sensor
7 | Knock sensor
8 | HO2S (Front, rear)
9 | PSP switch
10 | VSS
11 | Neutral switch
12 | Clutch switch
13 | Brake switch
14 | A/C switch, refrigent pressure switch (A/C operation request signal)
15 | Refrigent pressure switch (A/C compressor load signal)
16 | Generator
17 | TEN terminal (DLC)
18 | Battery
19 | IAC valve
20 | VIS control solenoid valve
21 | Variable tumble control solenoid valve
22 | Fuel injector
23 | Fuel pump relay
24 | Ignition coil
25 | Purge solenoid valve
26 | EGR valve
27 | HO2S sensor heater (Front, rear)
28 | A/C relay
29 | Fun control module
30 | Generator
31 | Combination meter (Water temperature gauge, Generator warning light, Drive information system display)
32 | IAC
33 | VIS
34 | VTCS
35 | Fuel injection control
36 | Fuel pump control
37 | ESA
38 | Purge control
39 | EGR control
40 | HO2S heater (Front, rear) control
41 | A/C cut-off control
42 | Electric fan control
43 | Generator control
44 | Information function