#
POWER SEAT SWITCH INSPECTION

BME091357155201

1. Disconnect the power seat switch connector.

2. Remove the seat back trim. (See FRONT SEAT DISASSEMBLY/ASSEMBLY.)

3. Disconnect the recliner motor connector.

4. Remove the seat cushion trim. (See FRONT SEAT DISASSEMBLY/ASSEMBLY.)

5. Disconnect the rear tilt motor connector.

6. Inspect for continuity between the power seat switch, recliner motor connector, and rear tilt motor connector terminals using an ohmmeter.

  • If not as specified, replace the power seat switch.