#
HEADLIGHT BULB REMOVAL/INSTALLATION

BME091851030W01

  Caution

  • A halogen bulb generates extremely high heat when it is used. If the surface of the bulb is soiled, excessive heat will build up and the light's life will be shortened. When replacing the bulb, hold the metal flange, not the glass.

1. Disconnect the negative battery cable.

2. Disconnect the headlight connector.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Cover
2 | Headlight bulb