#
AUTOMATIC TRANSAXLE SPECIFICATIONS [JA5A-EL]

BME050000000T08

Item | Specifications
--- | ---
For General (R.H.D.) specs. | Except for General (R.H.D.) specs.
Transaxle type | JA5A-EL
Engine type | AJ
Gear ratio | 1GR | 3.801
2GR | 2.131
3GR | 1.364
4GR | 0.935
5GR (O/D) | 0.685
Reverse | 2.970
Final gear ratio | 3.290 | 3.491
ATF | Type | ATF M-III or equivalent (e.g. Dexron®III)
Capacity (approximate quantity) (L {US qt, Imp qt}) | 9.7{10.3, 8.5}
Torque converter stall torque ratio | 1.86:1
Hydraulic system (Number of drive/driven plates) | Forward clutch | -
Coasting clutch | -
3-4 clutch | -
Low clutch | 7/7
2-4 brake | 3/4
High clutch | 5/5
Direct clutch | 4/4
Reverse clutch | 2/2
Low and reverse brake | 6/5
Band servo (mm {in}) | Servo diameter (Piston outer dia./retainer inner dia.) | -
Reduction accumulator piston outer dia./reduction band servo piston outer dia. | 49.66/57.64
Number of planetary gear teeth | Large sun gear | -
Small sun gear | -
Long pinion gear | -
Short pinion gear | -
Internal gear | -
Number of front planetary gear teeth | Ring gear | 74
Sun gear | 34
Pinion gear | 20
Number of rear planetary gear teeth | Ring gear | 75
Sun gear | 42
Pinion gear | 17
Number of reduction planetary gear teeth | Ring gear | 85
Sun gear | 31
Pinion gear | 27
Number of output gear teeth | 41
Number of idler gear teeth | 47
Number of reduction gear teeth | 23 | 22
Number of ring gear teeth | 66 | 67