#
CLUTCH HOUSING AND TRANSAXLE CASE COMPONENTS ASSEMBLY

BME051527100305

1. Assemble in the order indicated in the table.

1 | Oil passage
2 | Oil seal (differential) (See Oil Seal (Differential) Assembly Note.)
3 | Adjustment shim(s)
4 | Bearing race (differential) (See Bearing Race (Differential) Assembly Note.)
5 | Adjustment shim(s)
6 | Bearing race (transaxle case) (See Bearing Race (Transaxle Case) Assembly Note.)
7 | Drain plug and washer
8 | Reverse lever
9 | Reverse lever shaft
10 | Bearing race (differential) (See Bearing Race (Differential) Assembly Note.)
11 | Oil seal (differential) (See Oil Seal (Differential) Assembly Note.)
12 | Hole cover
13 | Bleeder
14 | Bleeder cover component
15 | Oil seal (change rod component) (See Oil Seal (Change Rod Component) Assembly Note.)
16 | Selector
17 | Boot (See Boot Assembly Note.)
18 | Change rod
19 | Roll pin
20 | Change arm
21 | Guide plate component
22 | Funnel
23 | Bearing race (secondary shaft)
24 | Oil seal (primary shaft) (See Oil Seal (Primary Shaft) Assembly Note.)
25 | Bearing race (primary shaft)

## Oil Seal (Differential) Assembly Note

1. Apply transaxle oil to the new oil seal lip.

2. Install the oil seal using the SST.

## Bearing Race (Differential) Assembly Note

1. Install the adjustment shim(s) and install the bearing race using a suitable pipe.

## Bearing Race (Transaxle Case) Assembly Note

1. Install the adjustment shim(s) and install the bearing race using a suitable pipe.

## Oil Seal (Change Rod Component) Assembly Note

1. Apply transaxle oil to the new oil seal lip.

2. Install the oil seal using a suitable pipe.

  Outer diameter of pipe
  26.0 mm {1.02 in}

## Boot Assembly Note

1. Install the boot with the drain hole facing downward when mounted on the vehicle.

## Oil Seal (Primary Shaft) Assembly Note

1. Apply transaxle oil to outer circumference of the oil seal.

2. Install the new oil seal using a suitable pipe.