#
TRANSAXLE OIL INSPECTION [G15M-R]

BME051527001W01

1. Park the vehicle on level ground.

2. Remove the oil level plug and washer.

3. Verify that the oil is near the brim of the plug port.

  • If the oil level is lower than the low level, add the specified amount and type of oil through the oil level plug hole.

Oil grade

  API Service GL-4 or GL-5

Oil viscosity

  All-season: SAE 75W-90
  Above 10 °C {50 °F}: SAE 80W-90

4. Install a new washer and the oil level plug.

Tightening torque

  40-58 N·m {4.0-6.0 kgf·m, 29-43 ft·lbf}