#
POWER BRAKE UNIT REMOVAL/INSTALLATION

BME041143800202

1. For the L.H.D. model, remove the battery.

2. For the L.H.D. model, remove the air cleaner. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [AJ].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. For the L.H.D. model (MZR-CD (RF Turbo)), remove the brake pipes between the master cylinder and brake pipe joint.

4. For the R.H.D. model (AJ), remove the dynamic chamber. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [AJ].)

5. For the R.H.D. model (AJ), remove the cruise actuator. (See CRUISE ACTUATOR REMOVAL/INSTALLATION.)

6. Remove the master cylinder. (See MASTER CYLINDER REMOVAL/INSTALLATION.)

7. Remove in the order indicated in the table.

1 | Vacuum hose
2 | Snap pin
3 | Clevis pin
4 | Nut
5 | Fork
6 | Nut
7 | Power brake unit
8 | Gasket (R.H.D.)
9 | Spacer (R.H.D.)
10 | Gasket

8. Install in the reverse order of removal.