#
GLOW PLUG LEAD INSPECTION [MZR-CD (RF Turbo)]

BME011318611W01

1. Remove the glow plug lead from the glow plug. (See GLOW PLUG REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Verify that the glow plug lead is not broken or bent.

3. Verify there is continuity at both ends of the glow plug lead.

  • If there is no continuity, replace the glow plug lead.

  Note

  • When inspecting for continuity in the glow plug lead, do not let the uncovered parts (A) come into contact with other parts and be shorted.