#
POWER SLIDING DOOR (PSD) DRIVE MODULE REMOVAL/INSTALLATION

BME091100155201

1. Remove the rear side trim.

2. Remove the woofer. (LH only)

3. Remove the rear A/C unit. (RH only) (SeeREAR A/C UNIT REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

1 | Cable (See Cable Removal Note) (See Cable Installation Note)
2 | Front pulley
3 | Rear pulley
4 | PSD drive module

## Cable Removal Note

1. While pulling the front pulley cable fully, pull the adjustment hook.

2. Open the sliding door.

3. While slightly lifting up the sliding door, remove the cables from the center roller.

## Cable Installation Note

1. Draw the rear cable outside of the compartment by passing them through the pulley installation holes, then install the rear pulley.

2. Install the rear cable end to the center roller.

  Caution

  • The following procedure is for the cable play adjustment. If the cable play is not adjusted correctly, the PSD system may not operate properly.

3. While pulling the front cable tube at 49 N {5.0 kgf, 11 lbf} or more, press in the adjustment hook.

4. Verify that the length of the metal part of the front cable tube is 18 mm {0.71 in} or more.

  • If it is less than 18 mm {0.71 in}, adjust the cable play again.