#
TRANSAXLE OIL INSPECTION [A65M-R]

BME051527001203

1. Park the vehicle on level ground.

2. Remove the filler plug and gasket.

3. Verify that the oil is near the brim of the plug port.

  • If the oil level is low, add the specified amount and type of oil through the filler plug hole.

Oil grade

  API Service GL-4 or GL-5

Oil viscosity

  SAE 75W-90

4. Install a new gasket and the filler plug.

Tightening torque

  30.0-39.0 N·m {3.06-3.98 kgf·m, 22.1-28.8 in·lbf}