#
SLIDING DOOR DISASSEMBLY/ASSEMBLY

BME091173002W02

1. Operate the rear door glass so that the distance from the top of the rear door glass to the upper part of the rear beltline molding is 260 mm {10 in}.

2. Disconnect the negative battery cable.

3. Remove the sliding door trim.

4. To remove the rear door glass, remove the rear beltline molding.

5. Disassemble in the order indicated in the table.

6. Assemble in the reverse order of disassembly.

1 | Door screen
2 | Door lock knob
3 | Glass guide
4 | Rear door glass (See Rear Door Glass Disassembly Note)
5 | Glass run channel
6 | Rear manual window regulator
7 | Rear power window regulator
8 | Remote controller
9 | Sliding door lock
10 | Outer handle
11 | Sliding door circuit contact
12 | Upper roller
13 | Center roller
14 | Lower roller
15 | Open lock

## Rear Door Glass Disassembly Note

1. Remove the rear beltline molding.

2. Remove the rear door glass installation bolts.

3. To remove the rear door glass from the glass run channel, lower the rear door glass.

4. Set the rear door glass in the notches of the sliding door, and pull it out while tilting it forward.