#
STARTER REMOVAL/INSTALLATION [AJ]

BME011918400203

  Warning

  • When the battery cables are connected, touching the vehicle body with starter terminal B will generate sparks. This can cause personal injury, fire, and damage to the electrical components. Always disconnect the battery negative cables before performing the following operation.

1. Remove the battery.

2. Remove the air cleaner.

3. Disconnect the selector cable. (See SELECTOR LEVER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Terminal B wire
2 | Terminal S wire
3 | Starter

5. Install in the reverse order of removal.