#
PRECAUTION (STEERING)

BME061000000W01

## Wheels and Tires Removal/Installation

1. When a wheel is installed, tighten it to

89-117 N·m {9.0-12.0 kgf·m, 66-86 ft·lbf}.

## Power Steering Components Removal/Installation

1. If any power steering fluid line has been disconnected anytime during the procedure, add ATF M-III or equivalent (e.g. DexronII), bleed the fluid lines, and inspect for leakage after the procedure has been completed.

## Connectors Disconnection/Connection

1. Disconnect the negative battery cable before doing any work that requires handling of connectors. Reconnect the negative battery cable only after the work is completed.