#
TRANSAXLE OIL REPLACEMENT [G15M-R]

BME051527001202

1. Park the vehicle on level ground.

2. Remove the drain plug with the washer.

3. Drain the oil into a suitable container.

4. Install a new washer and the drain plug.

Tightening torque

  40-58 N·m {4.0-6.0 kgf·m, 29-43 ft·lbf}

5. Remove the oil level plug with washer and add the specified amount and type of oil through the oil level plug hole until the level reaches the bottom of the oil level plug hole.

Oil grade

  API Service GL-4 or GL-5

Oil viscosity

  All-season: SAE 75W-90
  Above 10 °C {50 °F}: SAE 80W-90

Capacity (approx. quantity)

  2.70 L {2.85 US qt, 2.38lmp qt}

6. Install a new washer and the oil level plug.

Tightening torque

  40-58 N·m {4.0-6.0 kgf·m, 29-43 ft·lbf}