#
DTC P0711 [FN4A-EL]

BME050201030208

DTC P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (stuck)
--- | ---
DETECTION CONDITION | • If all conditions below are satisfied, the PCM determines that there is a malfunction.

  - When 180 s have passed after engine is started, vehicle is driven for 150 s or more at a speed of between 25-59 km/h {15-36 mph}, then 60 km/h {37 mph} or more for 100 s or more.
  - P0712, P0713 is not output.
  - Variation in ATF voltage is below 0.06 V.

Diagnostic support note:
• This is a continuous monitor (CCM).
• The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• The PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle.
• FREEZE FRAME DATA is available.
• The HOLD indicator light flashes.
• The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • TFT sensor malfunction • Connector corrosion • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has the FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Bulletins and or/on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT TFT SENSOR VOLTAGE • Turn the ignition switch to the LOCK position. • Connect the breakout box to the PCM. • Turn the ignition switch to the ON position (engine off). • Inspect the voltage at PCM terminal 3D.
• Record the terminal 3D voltage.
• Start the engine.
• Drive the vehicle at 60 km/h {37 mph} or more for 430 s or more.
• Record the terminal 3D voltage again.
• Is the variation in voltage 0.06 V or more?
Yes
Go to Step 5.
No | Go to the next step.
4 | INSPECT TERMINAL CONDITION • Turn the ignition switch to the LOCK position. • Disconnect the ATX connector. • Inspect terminals for corrosion. • Are terminals normal? | Yes | Go to the next step.
No | Repair or replace the terminals, then go to the next step.
5 | VERIFY TROUBLESHOOTING OF DTC P0711 COMPLETED • Make sure to reconnect all the disconnected connectors. • Clear the DTC from the memory using the WDS or equivalent. • Decrease ATF temperature to 20 °C {68 °F} or less. • Start the engine and wait for 180 s or more.
• Drive the vehicle at a speed between 25-59 km/h {15-36 mph} for 150 s or more.
• Drive the vehicle at a speed of 60 km/h {37 mph} or more for 100 s or more.
• Is the PENDING CODE present?
Yes
Replace the PCM, then go to the next step.
(See PCM REMOVAL/INSTALLATION [L3].)
No | Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [FN4A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [FN4A-EL].)
No | DTC troubleshooting completed.