#
FRONT FLOOR COVERING REMOVAL/INSTALLATION

BME091768670W01

## Fixed type Second-Row Seat

1. Disconnect the negative battery cable.

2. Remove the front seats. (See SECOND-ROW SEAT REMOVAL.)

3. Remove the second-row seat.

4. Remove the front scuff plates.

5. Remove the rear scuff plates.

6. Remove the console lower covers.

7. Remove the rear console.

8. Remove the front side trims.

9. Remove the B-pillar lower trims.

10. Remove the lower anchor of the front seat belt installation bolts.

11. Remove the trunk side trims.

12. Remove the adapter cover.

13. Remove the rear heater grilles.

14. Remove the parking brake cover.

15. Remove the rear heat duct. (for second-row seat)

16. Remove the fasteners.

17. Remove the front floor covering from the vehicle through the passenger-side front door.

18. Install in the reverse order of removal.

## Side-Sliding type Second-Row Seat

1. Disconnect the negative battery cable.

2. Remove the front seats.

3. Remove the second-row seats. (See SECOND-ROW SEAT REMOVAL.)

4. Remove the front scuff plate.

5. Remove the rear scuff plate.

6. Remove the console lower cover.

7. Remove the front side trim.

8. Remove the B-pillar lower trim.

9. Remove the lower anchor of the front seat belt installation bolt.

10. Remove the rear side trim.

11. Remove the long slider cover and adapter cover. (See LONG SLIDER AND ADAPTER REMOVAL/INSTALLATION.)

12. Remove the child restraint seat anchor cover.

13. Remove the rear heater grilles.

14. Remove the parking brake cover.

15. Remove the rear heat duct. (For second-row seat)

16. Remove the fasteners, and remove the floor covering.

17. Remove the floor covering from the vehicle through the passenger-side front door.

18. Install in the reverse order of removal.