#
DTC P0500 [MZR-CD (RF Turbo)]

BME010200102275

DTC P0500 | VSS circuit problem
--- | ---
DETECTION CONDITION | • The PCM monitors the vehicle speed signal from the ABS, ABS/TCS HU/CM. If the vehicle speed signal is not correct, the PCM determines that the vehicle speed signal from ABS, ABS/TCS HU/CM has malfunction. Diagnostic support note • The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• PENDING CODE is available if the PCM detects the above malfunction condition during the first drive cycle.
• FREEZE FRAME DATA is available.
• The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • ABS, ABS/TCS HU/CM malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related service repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | VERIFY CURRENT INPUT SIGNAL STATUS: IS CONCERN INTERMITTENT OR CONSTANT? • Connect the WDS or equivalent to the DLC-2. • Start the engine. • Access the VSS PID. • Read the VSS PID when the vehicle is driving.
• Is the VSS PID normal?
Yes
Intermittent concern exists.
Perform the "INTERMITTENT CONCERN TROUBLESHOOTING".
(See INTERMITTENT CONCERN TROUBLESHOOTING [MZR-CD (RF Turbo)].)
No | Go to the next step.
4 | INSPECT ABS, ABS/TCS HU/CM • Inspect the ABS, ABS/TCS HU/CM. (See ABS HU/CM INSPECTION.) • Is there any malfunction? | Yes | Repair or replace the malfunctioning part, then go to the next step.
No | Go to the next step.
5 | VERIFY TROUBLESHOOTING OF DTC P0500 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Drive the vehicle under the FREEZE FRAME DATA condition. • Is the PENDING CODE same as the DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)
No | Go to the next step.
6 | VERIFY AFTER REPAIR PROCEDURE • Perform the Repair Verification Drive Mode. (See OBD DRIVE MODE [MZR-CD (RF Turbo)].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | DTC troubleshooting completed.