#
CLUTCH HOUSING AND TRANSAXLE CASE COMPONENTS DISASSEMBLY

BME051517010301

1. Disassemble in the order indicated in the table.

1 | Bearing race (primary shaft)
2 | Oil seal (primary shaft) (See Oil Seal (Primary Shaft) Disassembly Note.)
3 | Bearing race (secondary shaft) (See Bearing Race (Secondary Shaft) Disassembly Note.)
4 | Funnel
5 | Guide plate component
6 | Change arm
7 | Roll pin (See Roll Pin Disassembly Note.)
8 | Change rod
9 | Boot
10 | Selector
11 | Oil seal (change rod component) (See Oil Seal (Change Rod Component) Disassembly Note.)
12 | Bleeder cover component
13 | Bleeder
14 | Hole cover
15 | Oil seal (differential) (See Oil Seal (Differential) Disassembly Note.)
16 | Bearing race (differential) (See Bearing Race (Differential) Disassembly Note.)
17 | Reverse lever shaft (See Reverse Lever Shaft Disassembly Note.)
18 | Reverse lever
19 | Drain plug and washer
20 | Bearing race (transaxle case) (See Bearing Race (Transaxle Case) Disassembly Note.)
21 | Adjustment shim(s)
22 | Bearing race (differential) (See Bearing Race (Differential) Disassembly Note.)
23 | Adjustment shim(s)
24 | Oil seal (differential) (See Oil Seal (Differential) Disassembly Note.)
25 | Oil passage

## Oil Seal (Primary Shaft) Disassembly Note

1. Remove the oil seal using the flathead screwdriver.

## Bearing Race (Secondary Shaft) Disassembly Note

1. Remove the bearing race by lifting it and the funnel out together.

## Roll Pin Disassembly Note

1. Align the groove for removal of the clutch housing pin with the position of the roll pin, then tap the pin out using a pin punch.

## Oil Seal (Change Rod Component) Disassembly Note

1. Remove the oil seal using the flathead screwdriver.

## Oil Seal (Differential) Disassembly Note

1. Remove the oil seal using the flathead screwdriver.

## Bearing Race (Differential) Disassembly Note

1. Remove the bearing outer race using the SST.

## Reverse Lever Shaft Disassembly Note

1. Remove the roll pin using the pliers.

2. Protect the reverse lever shaft with a rag and remove the shaft using the pliers.

## Bearing Race (Transaxle Case) Disassembly Note

1. Remove the bearing race using the SST.