#
NO.13 NO KICKDOWN [JA5A-EL]

BME050301030249

13 | No kickdown
DESCRIPTION | • Does not downshift when accelerator pedal is fully depressed within kickdown range.
POSSIBLE CAUSE | • If transaxle does not downshift though shifting is normal, the malfunction is in the TP sensor circuit (including sensor ground, sensor harness and connector).

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.