#
DTC 06 ERR02 OR 06:ER02

BME090266900W21

DTC 06 ERR02 or 06:Er02 | CD changer (upper module)
DETECTION CONDITION |

  Note

  • When error occurs, error message "CHECK CD" is displayed in the LCD.

• Cannot play CD normally or change tracks.
POSSIBLE CAUSE | • Defective CD (scratches or dirt) • CD changer (upper module) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY WHETHER MALFUNCTION IS IN CD CHANGER (UPPER MODULE) OR CD • Play all CDs in changer and select other song (change tracks). • Is CD changer able to change tracks? | Yes | Go to Step 3.
No | Not able to change particular tracks. | Go to next step.
Not able to change any tracks. | Change CD and perform track-change again. • If CD changer changes tracks, go to Step 3. • If not, replace CD changer (upper module).
2 | INSPECT CD • Inspect condition of CD where error has occurred. • Is CD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace CD, then go to next step.
3 | INSPECT CD CHANGER (UPPER MODULE) • Clear DTC. • Play CD and select other song (change tracks). • Start on-board diagnostic test mode. • Is DTC 06 ERR02 or 06:Er02 displayed? | Yes | Replace CD changer (upper module).
No | Troubleshooting completed.