#
REAR HEAT DUCT COMPONENT REMOVAL/INSTALLATION

BME071161273W01

## For Second-row Seat

1. Remove the front seat.

2. Turn floor covering over.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Rear duct
2 | Rear heat duct No.1
3 | Rear heat duct No.2
4 | Rear heat duct No.3

## For Third-row Seat

### Rear heat duct No.4

1. Disconnect the negative battery cable.

2. Remove the third-row seat.

3. Remove the right side trunk side trim.

4. Remove as indicated in the table.

5. Install in the reverse order of removal.

1 | Rear heat duct No.4

### Rear heat duct No.5

1. Disconnect the negative battery cable.

2. Fold the third-row seat into rear space.

3. Remove the right side trunk side trim.

4. Remove the rear heat duct No.4.

5. Remove the rear heater grilles.

6. Turn the front floor covering over.

7. Remove in the order indicated in the table.

8. Install in the reverse order of removal.

1 | Rear heat duct No.5