#
CALIPER (FRONT) DISASSEMBLY/ASSEMBLY

BME041133990W01

1. Disassemble in the order indicated in the table.

1 | Dust seal
2 | Piston (See Piston Disassembly Note)
3 | Piston seal (See Piston Seal Disassembly Note)
4 | Bleeder cap
5 | Bleeder screw
6 | Caliper

2. Assemble in the reverse order of removal.

## Piston Disassembly Note

  Caution

  • Blow the compressed air slowly to prevent the piston from suddenly popping out.

1. Place the SST in the caliper, then blow compressed air through the hole to force the piston out of the caliper.

## Piston Seal Disassembly Note

1. Remove the piston seal from the brake caliper using the SST.