#
ELECTRICAL SYSTEM

BME000000006601

## Connectors

### Disconnecting connectors

  • When disconnecting connector, grasp the connectors, not the wires.
  • Connectors can be disconnected by pressing or pulling the lock lever as shown.

### Locking connector

  • When locking connectors, listen for a click indicating they are securely locked.

### Inspection

  • When a tester is used to inspect for continuity or measuring voltage, insert the tester probe from the wiring harness side.
  • Inspect the terminals of waterproof connectors from the connector side since they cannot be accessed from the wiring harness side.

  Caution

  • To prevent damage to the terminal, wrap a thin wire around the tester probe before inserting into terminal.